# Encapsulant

## HPCS EN HazMat Gel - Hazardous Material Encapsulant

EN HazMat Gel Hazardous Material Encapsulant product label

**EN HazMat Gel** is used to encapsulate dust from hazard materials such as lead and asbestos. After removal of hazardous material, plaster can be "locked down" with the **EN Haz-Mat Gel**. Precede application with **HPCS CO S-50 Primer** (prepared from HPCS CO R-100 BASE and CO Converter).



[Download the EN HazMat Gel Technical Data Sheet](http://ww2.historicplaster.com/wp-content/uploads/2020/10/EN-HazMat-Gel-Technical-Data-Sheet.pdf)

[Download the EN HazMat Gel Safety Data Sheet](http://ww2.historicplaster.com/wp-content/uploads/2020/10/EN-HazMat-Gel-Safety-Data-Sheet.pdf)

[content\_block slug=product-disclaimer]