# Reinforcement

## HPCS RE Aramid Gel™ for Reinforcing and Stabilizing Fibrous Plaster

RE Aramid Gel Fiber Reinforced Plaster Rebuilder product label

**Fiber\* Reinforced Plaster Rebuilder Reinforced with DuPont™ KEVLAR®**

Used to reinforce fractured cast fibrous plaster panels in suspended ceiling systems. Use with appropriate HPCS primer – **CO S-50**or **CO S-20**.

Ideal for rebuilding damaged cast plaster ceiling panels and establishing new structural support hooks without causing surface damage.

*\*DuPont™ and KEVLAR® are registered trademarks of E.I. du Pont de Nemours and Company and are used with permission.*

https://youtu.be/mqyyG2zdqcY

[Download the RE Aramid Gel Technical Data Sheet PDF](http://ww2.historicplaster.com/wp-content/uploads/2020/10/RE-Aramid-Gel-Technical-Data-Sheet.pdf)

[Download the RE Aramid Gel Safety Data Sheet (EN)](http://ww2.historicplaster.com/wp-content/uploads/2020/10/RE-Aramid-Gel-Safety-Data-Sheet-EN.pdf)

[Download the RE Aramid Gel Safety Data Sheet (FR)](http://ww2.historicplaster.com/wp-content/uploads/2020/10/RE-Aramid-Gel-Safety-Data-Sheet-FR.pdf)

[content\_block slug=product-disclaimer]